INSPECTION AFTER REMOVAL

- Check that insulator on the top surface of fuel tank protector (LH) has no peeling or displacement.

- If insulator has a peeling or displacement, replace insulator, referring to the figure.

  1 | : Insulator (RH)
  2 | : Fuel tank protector (LH)
  3 | : Insulator (LH)
  a | : 20 mm (0.79 in)
  | : Vehicle front

- Check that there is no malfunction on the baffle plate in the fuel tank.

INSPECTION AFTER INSTALLATION
Use the following procedure to check for fuel leakage.

1.Turn ignition switch “ON” (with engine stopped), and check connections for leakage by applying fuel pressure to fuel piping.

2.Start engine and rev it up and check there are no fuel leakage at the fuel system tube and hose connections.

- After removing/installing rear suspension assembly, check and adjust the wheel alignment. Refer to Inspection.