DTC DETECTION LOGIC

DTC | Self-diagnosis name | DTC detection condition | Possible cause
P0712 | Transmission fluid temperature sensor "A" circuit low | A DTC is set if the fluid temperature sensor voltage value received by TCM is less than 39 mV. |

- Fluid temperature sensor
- Harness or connector
  (Open or shorted in the fluid temperature sensor circuit)

DTC CONFIRMATION PROCEDURE
1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE
With CONSULT-III

1. Start the engine and run at idle for 5 seconds or more.
2. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Start the engine and run at idle for 5 seconds or more.
2. Check self-diagnosis.

Is DTC P0712 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident.