Work after rear fender and lock pillar reinforcement are removed. Remove the outer sill reinforcement rear and rear pillar reinforcement (reusable).

1. | Outer sill reinforcement rear | 2. | Rear pillar reinforcement | 3. | Outer rear sill brace
4. | Urethane foam | 5. | Highly rigid foaming agent |  |
Unit: mm (in) |  |  |  |
: Vehicle front |  |  |  |
Replaced parts
• | Outer rear wheelhouse (LH) |  |  |  |

■ CAUTION ■
Refer to Foam Repair (section of Example of highly rigid foaming agent repair procedure) for filling procedure of highly rigid foaming agent.

1. | Outer sill reinforcement rear | 2. | Rear pillar reinforcement | 3. | Outer rear sill brace
: Vehicle front |  |  |  |

View D: Before installing outer sill reinforcement rear
View H: Before installing rear pillar reinforcement