■ CAUTION ■

- Never apply any chemical products like wax, coating agent, and compound for carbon parts. They are produced by composite manufacturing methods similar to a racing vehicle and special paint is adopted to enhance the look and feel of materials. (Otherwise, water may penetrate to carbon layers and may cause corrosion.)
- Never place any carbon parts directly on the ground. Always protect them using a soft sheet during removal, installation, and replacement operations.Never touch carbon parts with oily hands or allow oil or grease to get on them.

REMOVAL
Rear diffuser (center)

1.Remove the clips connecting with the rear bumper fascia (lower) lower surface.

2.Remove the rear diffuser (center) mounting bolts.

3.Remove the rear diffuser (center).

Rear diffuser RH

1.Remove the rear diffuser (center).

2.Remove the mounting bolts and clips of rear diffuser RH.

3.Remove the rear diffuser RH.

Rear diffuser LH

1.Remove the rear diffuser (center).

2.Remove the mounting bolts and clips of rear diffuser LH.

3.Remove the rear diffuser LH.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- When rear diffuser mounting bolt is removed, check for surface treatment peel off and oxidation of mounting bolt and washer so that electric corrosion is prevented.
- Regarding mounting bolt and washer with surface treatment peel off, paint contact surface of washer and carbon using touch pen or others. By doing so, mounting bolt and washer are reusable. However, regarding oxidation, never reuse.
- Visually check the clips for deformation and damage at installation. Replace with new ones if necessary.
- Always tighten the mounting bolts to the specified torque.