WORK SUPPORT

Service item | Setting item | Setting
SET I/L D-UNLCK INTCON | ON* | With the interior room lamp timer function
OFF | Without the interior room lamp timer function
ROOM LAMP TIMER SET | MODE 2 | 7.5 sec. | Sets the interior room lamp ON time. (Timer operating time)
MODE 3* | 15 sec.
MODE 4 | 30 sec.
ROOM LAMP ON TIME SET | MODE 1 | 0.5 sec. | Sets the interior room lamp gradual brightening time.
MODE 2* | 1 sec.
MODE 3 | 2 sec.
MODE 4 | 3 sec.
MODE 5 | 0 sec.
ROOM LAMP OFF TIME SET | MODE 1 | 0.5 sec. | Sets the interior room lamp gradual dimming time.
MODE 2 | 1 sec.
MODE 3 | 2 sec.
MODE 4* | 3 sec.
R LAMP TIMER LOGIC SET | MODE 1* | Interior room lamp timer activates with synchronizing all doors.
MODE 2 | Interior room lamp timer activates with synchronizing the driver door only.
*: Factory setting

DATA MONITOR

Monitor item [Unit] | Description
REQ SW-DR [On/Off] | The switch status input from request switch (driver side)
REQ SW-AS [On/Off] | The switch status input from front request switch (passenger side)
REQ SW-RR [On/Off] | NOTE： The item is indicated, but not monitored.
REQ SW-RL [On/Off] | NOTE： The item is indicated, but not monitored.
PUSH SW [On/Off] | The switch status input from push-button ignition switch
ACC RLY-F/B [On/Off] | NOTE： The item is indicated, but not monitored.
KEY SW-SLOT [On/Off] | Key switch status input from key slot
UNLK SEN-DR [On/Off] | Driver door unlock status input from unlock sensor
DOOR SW-DR [On/Off] | The switch status input from driver side door switch
DOOR SW-AS [On/Off] | The switch status input from passenger side door switch
DOOR SW-RR [On/Off] | NOTE： The item is indicated, but not monitored.
DOOR SW- RL [On/Off] | NOTE： The item is indicated, but not monitored.
DOOR SW-BK [On/Off] | NOTE： The item is indicated, but not monitored.
CDL LOCK SW [On/Off] | Lock switch status received from the door lock and unlock switch
CDL UNLOCK SW [On/Off] | Unlock switch status received from the door lock and unlock switch
KEY CYL LK-SW [On/Off] | NOTE： The item is indicated, but not monitored.
KEY CYL UN-SW [On/Off] | NOTE： The item is indicated, but not monitored.
TRNK/HAT MNTR [On/Off] | The switch status input from trunk room lamp switch
RKE-LOCK [On/Off] | Lock signal status received from remote keyless entry receiver
RKE-UNLOCK [On/Off] | Unlock signal status received from remote keyless entry receiver

ACTIVE TEST

Test item | Operation | Description
INT LAMP | On | Outputs the interior room lamp control signal to turn map lamp ON (Map lamp switch is in DOOR position).
Off | Stops the interior room lamp control signal to turn map lamp OFF.
STEP LAMP TEST | On | Outputs the step lamp control signal to turn step lamp ON.
Off | Stops the step lamp control signal to turn step lamp OFF.
LUGGAGE LAMP TEST | On | Outputs the trunk room lamp control signal to turn the trunk room lamp ON.
Off | Stops the trunk room lamp control signal to turn the trunk room lamp OFF.