REMOVAL

1.Remove the clip (A) from the front edge of the center mud guard.

2.Remove the clip (A) from the rear edge of the center mud guard.

3.Remove the mounting screws on the center mud guard lower surface.

4.Fully open the door.

5.Disengage the clips of the center mud guard (1) from vehicle rear sequentially with the remover tool (A).
■ CAUTION ■
Apply protective tape (B) to the body side to protect from damage.

6.Remove the center mud guard from the vehicle body.

7.Remove the mounting screws after removing the center mud guard, and then remove the front bracket, center bracket, rear bracket, and wind deflector from the vehicle body.
NOTE：
The front bracket, center bracket, rear bracket, and wind deflector can be removed as a single part.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- Check visually the clips for deformation and damage at installation. Replace with new ones if necessary.
- When installing, check that the clips are accurately aligned with the body side panel, then press in.