DTC DETECTION LOGIC

DTC | Display Item | Malfunction detected condition | Possible causes
C1728 | RECEIVER ID NO REG | Receiver ID registration cannot be performed. |

- Tire pressure receiver malfunction
- Low tire pressure warning control unit malfunction

DTC REPRODUCTION PROCEDURE
1.DTC REPRODUCTION PROCEDURE
With CONSULT-III

1. Drive for 3 minutes at a speed of 40 km/h (25 MPH) or more, then drive normally for 10 minutes.
2. Perform self-diagnosis of the low tire pressure warning control unit.

Is DTC “C1728” detected?
YES>>Perform trouble diagnosis. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END