PREPARATION BEFORE ADJUSTING NOTE：

- For details, refer to the regulations in your own country.
- Perform aiming if the vehicle front body has been repaired and/or the headlamp assembly has been replaced.

Before performing aiming adjustment, check the following.

- Adjust the tire pressure to the specification.
- Fill with fuel, engine coolant and each oil.
- Maintain the unloaded vehicle condition. (Remove luggage from the passenger compartment and the trunk room.)
  NOTE：
  Do not remove the temporary tire, jack and on-vehicle tool.
- Wipe out dirt on the headlamp.
  ■ CAUTION ■
  Never use organic solvent (thinner, gasoline etc.)
- Ride alone on the driver seat.

AIMING ADJUSTMENT SCREW

A | Headlamp (RH) UP/DOWN adjustment screw | B. | Headlamp (LH) UP/DOWN adjustment screw |  |
: Vehicle center

Adjustment screw | Screw driver rotation | Facing direction
A | Headlamp (RH) UP/DOWN | Clockwise | DOWN
Counterclockwise | UP
B | Headlamp (LH) UP/DOWN | Clockwise | DOWN
Counterclockwise | UP