VALUES ON THE DIAGNOSIS TOOL CONSULT-III MONITOR ITEM

Monitor Item | Condition | Value/Status
VHCL SPD SIG | Ignition switch ON | Vehicle speed > 0 km/h (0 MPH) | On
Vehicle speed = 0 km/h (0 MPH) | Off
PKB SIG | Ignition switch ON | Parking brake is applied. | On
Parking brake is released. | Off
ILLUM SIG | Ignition switch ON | Light switch ON | On
Light switch OFF | Off
IGN SIG | Ignition switch ON | — | On
Ignition switch ACC | — | Off
REV SIG | Ignition switch ON | Selector lever in R position | On
Selector lever in any position other than R | Off
SIDE VIEW SW | Ignition switch ON | This item is displayed, but cannot be monitored. | Off
ROOM LAMP | Ignition switch ON | This item is displayed, but not used. | Off

TERMINAL LAYOUT
PHYSICAL VALUES

Terminal (Wire color) | Description | Condition | Reference value (Approx.)
+ | – | Signal name | Input/Output
1 (V) | Ground | BOSE amp. ON signal | Output | Ignition switch ON | — | 12.0 V
2 (R) | 3 (P) | Audio signal front LH | Output | Ignition switch ON | Sound output |
4 (V) | 5 (W) | Audio signal rear LH | Output | Ignition switch ON | Sound output |
6 (V) | 15 (GR) | Steering switch signal A | Input | Ignition switch ON | Keep pressing SOURCE switch. | 0 V
Keep pressing SEEK switch to . | 1.0 V
Keep pressing SEEK switch to . | 2.0 V
Keep pressing switch. | 3.0 V
Keep pressing START / STOP switch. | 4.0 V
Except for above. | 5.0 V
7 (V) | Ground | ACC power supply | Input | Ignition switch ACC | — | Battery voltage
10 (GR) | — | Shield | — | — | — | —
11 (R) | 12 (G) | Audio signal front RH | Output | Ignition switch ON | Sound output |
13 (BR) | 14 (Y) | Audio signal rear RH | Output | Ignition switch ON | Sound output |
16 (SB) | 15 (GR) | Steering switch signal B | Input | Ignition switch ON | Keep pressing VOL switch to -. | 0 V
Keep pressing VOL switch to +. | 1.0 V
Keep pressing switch. | 2.0 V
Keep pressing MRK switch. | 3.0 V
Except for above. | 5.0 V
19 (Y) | Ground | Battery power supply | Input | Ignition switch OFF | — | Battery voltage
20 (B) | Ground | Ground | — | Ignition switch ON | — | 0 V
26 (G) | Ground | AUX image signal | Input | Ignition switch ON | At AUX image is displayed. |
29 (SB) | Ground | Disk eject signal | Input | Ignition switch ON | Pressing the eject switch. | 0 V
Except for above. | 5.0 V
46 (R) | Ground | AUX image signal ground | — | Ignition switch ON | — | 0 V
47 | — | Shield | — | — | — | —
49 (BR) | Ground | Switch ground | — | Ignition switch ON | — | 0 V
65 (R) | Ground | Parking brake signal | Input | Ignition switch ON | Parking brake is ON. | 4.5 V
Parking brake is OFF. | 0 V
67 (W) | Ground | Composite image ground | — | Ignition switch ON | — | 0 V
68 (R) | Ground | Composite image signal | Output | Ignition switch ON | At DVD image is displayed. |
72 (L) | Ground | Microphone VCC | Output | Ignition switch ON | — | 5.0 V
73 (V) | Ground | Communication signal (CONT→DISP) | Output | Ignition switch ON | When adjusting display brightness. |
74 (P) | — | CAN–L | Input/Output | — | — | —
75 (R) | — | AV communication signal (L) | Input/Output | — | — | —
76 (R) | — | AV communication signal (L) | Input/Output | — | — | —
79 (R) | Ground | Illumination signal | Input | Ignition switch OFF | Lighting switch is OFF. | 0 V
Lighting switch is ON. | 12.0 V
80 (W) | Ground | Ignition signal | Input | Ignition switch ON | — | Battery voltage
81 (O) | Ground | Reverse signal | Input | Ignition switch ON | R position | 12.0 V
Other than R position | 0 V
82 (V) | Ground | Vehicle speed signal (8‐pulse) | Input | Ignition switch ON | When vehicle speed is approx. 40 km/h (25 MPH) | NOTE： Maximum voltage may be 12.0 V due to specifications (connected units).
83 | — | Shield | — | — | — | —
84 (B) | Ground | Composite synchronizing signal | Output | Ignition switch ON | — |
87 (P) | 71 | Microphone signal | Input | Ignition switch ON | Give a voice |
88 | — | Shield | — | — | — | —
89 (SB) | Ground | Communication signal (DISP→CONT) | Input | Ignition switch ON | When adjusting display brightness. |
90 (L) | — | CAN–H | Input/Output | — | — | —
91 (G) | — | AV communication signal (H) | Input/Output | — | — | —
92 (G) | — | AV communication signal (H) | Input/Output | — | — | —
104 (W) | 119 (B) | AUX sound signal LH | Input | Ignition switch ON | When AUX mode is selected. |
117 | — | Shield | — | — | — | —
118 (R) | 119 (B) | AUX sound signal RH | Input | Ignition switch ON | When AUX mode is selected. |
129 (G) | — | USB ground | — | — | — | —
130 (R) | — | USB D− | — | — | — | —
131 (W) | — | V BUS signal | — | — | — | —
132 (L) | — | USB D+ | — | — | — | —
133 | — | Shield | — | — | — | —
134 | Ground | Antenna amp. ON signal | Output | Ignition switch ON | — | 12.0 V
135 | — | AM–FM main | Input | — | — | —
136 | — | FM sub | Input | — | — | —
137 | Ground | GPS antenna signal | Input | Ignition switch ON | Not connected to GPS antenna connector | 5.0 V
138 | — | Shield | — | — | — | —
139 | Ground | Satellite radio antenna signal | Input | Ignition switch ON | Not connected to satellite radio antenna connector. | 5.0 V
140 | — | Shield | — | — | — | —
157 | Ground | RGB digital image signal (+) | Output | Ignition switch ON | Not connected connector. | 3.3 V
158 | Ground | RGB digital image signal (−) | Output | Ignition switch ON | Not connected connector. | 3.3 V