1.CHECK DOOR SWITCH

1. Turn ignition switch OFF.
2. Disconnect malfunctioning door switch connector.
3. Check continuity between door switch terminals.

   Terminal | Condition | Continuity
   Door switch
   2 | Ground part of door switch | Door switch | Pressed | Not existed
   Released | Existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace malfunction door switch. Refer to Removal and Installation.