APPLICATION ITEM CONSULT-III performs the following functions via CAN communication with BCM.

Diagnosis mode | Function Description
WORK SUPPORT | Changes the setting for each system function.
DATA MONITOR | The BCM input/output signals are displayed.
ACTIVE TEST | The signals used to activate each device are forcibly supplied from BCM.

DATA MONITOR

Monitored Item | Description
REQ SW -DR | Indicates [ON/OFF] condition of door request switch (driver side).
REQ SW -AS | Indicates [ON/OFF] condition of door request switch (passenger side).
REQ SW -RR | NOTE： This is displayed even when it is not equipped.
REQ SW -RL | NOTE： This is displayed even when it is not equipped.
REQ SW -BD/TR | Indicates [ON/OFF] condition of trunk lid opener request switch.
PUSH SW | Indicates [ON/OFF] condition of push-button ignition switch
UNLK SEN -DR | Indicates [ON/OFF] condition of driver door UNLOCK status.
KEY SW -SLOT | Indicates [ON/OFF] condition of key slot.
DOOR SW-DR | Indicates [ON/OFF] condition of front door switch LH.
DOOR SW-AS | Indicates [ON/OFF] condition of front door switch RH.
DOOR SW-RR | NOTE： This is displayed even when it is not equipped.
DOOR SW-RL | NOTE： This is displayed even when it is not equipped.
DOOR SW-BK | NOTE： This is displayed even when it is not equipped.
CDL LOCK SW | Indicates [ON/OFF] condition of lock signal from door lock/unlock switch LH and RH.
CDL UNLOCK SW | Indicates [ON/OFF] condition of unlock signal from door lock/unlock switch LH and RH.
KEY CYL LK-SW | NOTE： This is displayed even when it is not equipped.
KEY CYL UN-SW | NOTE： This is displayed even when it is not equipped.
KEY CYL SW-TR | NOTE： This is displayed even when it is not equipped.
TR/BD OPEN SW | Indicates [ON/OFF] condition of trunk lid opener switch.
TRNK/HAT MNTR | Indicates [ON/OFF] condition of trunk lid.
RKE-LOCK | Indicates [ON/OFF] condition of LOCK signal from Intelligent Key.
RKE-UNLOCK | Indicates [ON/OFF] condition of UNLOCK signal from Intelligent Key.
RKE-TR/BD | Indicates [ON/OFF] condition of TRUNK OPEN signal from Intelligent Key.

WORK SUPPORT

Test Item | Description
SECURITY ALARM SET | This mode is able to confirm and change security alarm ON-OFF setting.
THEFT ALM TRG | The switch which triggered vehicle security alarm is recorded. This mode is able to confirm and erase the record of vehicle security alarm. The trigger data can be erased by touching “CLEAR” on CONSULT-III screen.

ACTIVE TEST

Test Item | Description
THEFT IND | This test is able to check security indicator lamp operation. The lamp will be turned on when “ON” on CONSULT-III screen is touched.
VEHICLE SECURITY HORN | This test is able to check vehicle security horn operation. The horns will be activated for 0.5 seconds after “ON” on CONSULT-III screen is touched.
HEADLAMP(HI) | This test is able to check vehicle security lamp operation. The headlamps will be activated for 0.5 seconds after “ON” on CONSULT-III screen is touched.
FLASHER | This test is able to check vehicle security hazard lamp operation. The hazard lamps will be activated after “ON” on CONSULT-III screen is touched.