1.CHECK FUEL TANK TEMPERATURE SENSOR

1. Turn ignition switch OFF.
2. Disconnect “fuel level sensor unit and fuel pump (main)” harness connector.
3. Remove fuel level sensor unit.
4. Check resistance between “fuel level sensor unit and fuel pump (main)” terminals by heating with hot water as shown in the figure.

   Terminals | Condition | Resistance (kΩ)
   1 and 3 | Temperature　[°C (°F)] | 20 (68) | 2.3 - 2.7
   50 (122) | 0.79 - 0.90

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace “fuel level sensor unit and fuel pump (main)”.