1.CHECK CONDITION OF ALARM Operate alarm. Which alarm does not operate? Headlamp and horn >>GO TO 2. Headlamp>>GO TO 3.
Horn>>GO TO 4.
2.CHECK DOOR SWITCH
Check door switch.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 6.
NO>>Replace the malfunctioning door switch
3.CHECK HEADLAMP
Check headlamp operation.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 6.
NO>>Repair or replace malfunctioning parts.
4.CHECK HORN
Check horn.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 5.
NO>>Repair or replace malfunctioning parts.
5.CHECK VEHICLE SECURITY HORN
Check vehicle security horn.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 6.
NO>>Repair or replace malfunctioning parts.
6.CONFIRM THE OPERATION
Confirm the operation again.
Is the result normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.