Work after rear fender, rear panel, rear floor rear, rear floor side, lock pillar reinforcement, and outer rear wheelhouse are removed.

Unit: mm (in) |  |  |  |
: Vehicle front
Replacement parts
• | Rear side member assembly (LH) |  |  |  |

Unit: mm (in) |  |  |  |
: Vehicle front : Weld the parts onto the back of the component part.

View G: Before installing jack mounting bracket

Unit: mm (in) |  |  |  |
: Vehicle front : Weld the parts onto the back of the component part.