REMOVAL

1.Remove the front seat. Refer to Removal and Installation.

2.Remove the sliding switch escutcheon.

3.Remove the seat back trim and the seatback pad. Refer to Disassembly and Assembly.

4.Disconnect the sliding switch connector.

5.Remove the screws (A).

6.Remove the sliding switch (1) from the seat back frame (2).

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- When performing the work, use shop cloths to protect the parts from damage.
- Always fix the harness clamp in the normal position.