REMOVAL

1.Remove the console finisher assembly. Refer to Removal and Installation.

2.Remove the mounting screws (A) from the inside key antenna (instrument panel center).

3.Disconnect the inside key antenna (instrument panel center) connector, and then remove the inside key antenna (instrument panel center) (1) from the console finisher assembly (2).

INSTALLATION
Install in the reverse order of removal.