1.CHECK POWER WINDOW MAIN SWITCH (PASSENGER SIDE)

1. Turn ignition switch OFF.
2. Power window lock switch UNLOCK.
3. Disconnect power window main switch connector.
4. Check continuity between power window main switch terminals.

   Power window main switch | Condition | Continuity
   Connector | Terminal
   D8 | 6 | 2 | Passenger side switch | AUTO | Existed
   Other than above | Not existed
   7 | UP | Existed
   Other than above | Not existed
   15 | DOWN | Existed
   Other than above | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace power window main switch. Refer to Removal and Installation.