1.CHECK PUSH-BUTTON IGNITION SWITCH

1. Turn ignition switch OFF.
2. Disconnect push-button ignition switch connector.
3. Check continuity between push-button ignition switch terminals.

   Push-button ignition switch | Condition | Continuity
   Terminal
   1 | 4 | Push-button ignition switch | Pressed | Existed
   Not pressed | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace push-button ignition switch. Refer to Removal and Installation.