DTC DETECTION LOGIC

DTC | Self-diagnosis name | DTC detection condition | Possible cause
P2725 | Pressure control solenoid "E" electrical | A DTC is set if the lubricating flow solenoid valve monitor current value is less than 0.2 A when the lubricating flow solenoid valve target current value is more than 0.38 A. |

- Lubricating flow solenoid valve
- Harness or connector
  (Open or short in the lubricating flow solenoid valve circuit)

DTC CONFIRMATION PROCEDURE
1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE
With CONSULT-III

1. Start the engine.
2. Shift the shift lever to the P position and run at idle for 5 seconds or more.
3. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Start the engine.
2. Shift the shift lever to the P position and run at idle for 5 seconds or more.
3. Check self-diagnosis.

Is DTC P2725 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident.