1.CHECK TCM RELAY Check continuity between TCM relay connector terminals. ■ CAUTION ■

- When applying voltage, use a fuse.
- Never cause a short circuit.

TCM relay connector | Condition | Continuity
Connector | Terminal
B54 | 3 | 5 | Apply battery voltage between terminals 1 and 2 | Existed
Other than the above | Not existed
6 | 7 | Apply battery voltage between terminals 1 and 2 | Existed
Other than the above | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace TCM relay.