REMOVAL

1.Remove the door finisher. Refer to Removal and Installation.

2.Remove the inside handle cable from the inside handle. Remove the door lock knob cable from the door lock knob.
■ CAUTION ■
Never bend the cable end.

3.Remove the sealing screen and the door window. Refer to Removal and Installation (GT-R certified NISSAN dealer).

4.Remove the door inner west reinforcement. Refer to Exploded View.

5.Disengage the joint of key cylinder rod (driver side) and outside handle rod at the outside handle side.

6.Disconnect the door request switch connector.

7.Remove the TORX bolt of outside handle escutcheon by the arrow in the figure.

8.Pull out and remove the outside handle escutcheon (2) toward vehicle rear while pulling the outside handle (1) forward.
■ CAUTION ■
Never damage the vehicle.

9.Remove the TORX bolt by the arrows in the figure, and then remove the outside handle assembly.

10.Remove the TORX bolt and blind bolt, and then remove the key cylinder from the outside handle assembly. (Driver side)

INSTALLATION
Install in the reverse order of removal.
■ CAUTION ■

- When installing each rod, rotate rod holder until a click is felt.
- After installation, check door open/close, lock/unlock operation.