WORK SUPPORT

Service item | Setting item | Setting
BATTERY SAVER SET | On* | With the exterior lamp battery saver function
Off | Without the exterior lamp battery saver function
ILL DELAY SET | MODE 1 | NOTE： The item is indicated, but not operated.
MODE 2
MODE 3
MODE 4
MODE 5
MODE 6
MODE 7
MODE 8
*: Factory setting

DATA MONITOR

Monitor item [Unit] | Description
PUSH SW [On/Off] | The switch status input from push-button ignition switch
ENGINE STATE [Stop/Stall/Crank/Run] | The engine status received from ECM with CAN communication
VEH SPEED 1 [km/h] | The value of the vehicle speed received from combination meter with CAN communication
KEY SW-SLOT [On/Off] | Key switch status input from key slot
TURN SIGNAL R [On/Off] | Each switch status that BCM judges from the combination switch reading function
TURN SIGNAL L [On/Off]
TAIL LAMP SW [On/Off]
HI BEAM SW [On/Off]
HEAD LAMP SW1 [On/Off]
HEAD LAMP SW2 [On/Off]
PASSING SW [On/Off]
AUTO LIGHT SW [On/Off] | NOTE： The item is indicated, but not monitored.
FR FOG SW [On/Off] | NOTE： The item is indicated, but not monitored.
DOOR SW-DR [On/Off] | The switch status input from driver side door switch
DOOR SW-AS [On/Off] | The switch status input from passenger side door switch
DOOR SW-RR [On/Off] | NOTE： The item is indicated, but not monitored.
DOOR SW-RL [On/Off] | NOTE： The item is indicated, but not monitored.
DOOR SW-BK [On/Off] | NOTE： The item is indicated, but not monitored.

ACTIVE TEST

Test item | Operation | Description
TAIL LAMP | On | Transmits the position light request signal to IPDM E/R with CAN communication to turn the tail lamp ON.
Off | Stops the position light request signal transmission.
HEAD LAMP | Hi | Transmits the high beam request signal with CAN communication to turn the headlamp (HI).
Low | Transmits the low beam request signal with CAN communication to turn the headlamp (LO).
Off | Stops the high & low beam request signal transmission.
FR FOG LAMP | On | NOTE： The item is indicated, but cannot be tested.
Off
DAYTIME RUNNING LIGHT | On | Transmits the daytime running light request signal with CAN communication to turn the daytime running light.
Off | Stops the daytime running light request signal transmission.
CORNERING LAMP | RH | NOTE： The item is indicated, but cannot be tested.
LH
Off
ILL DIM SIGNAL | On | NOTE： The item is indicated, but cannot be tested.
Off