1.PERFORM CALIBRATION OF PRESSURE SENSOR Perform pressure sensor calibration. Refer to Special Repair Requirement (GT-R certified NISSAN dealer). >>GO TO 2. 2.PERFORM CALIBRATION OF VALVE Perform valve calibration. Refer to Special Repair Requirement (GT-R certified NISSAN dealer).
Is calibration of valve finished?
YES>>INSPECTION END
NO>>GO TO 3.
3.CHECK ABS ACTUATOR AND ELECTRIC UNIT (CONTROL UNIT)
Perform self-diagnosis for “ABS” with CONSULT-III.
Is DTC “C1193” detected?
YES>>Replace ABS actuator and electric unit (control unit). Refer to Exploded View (GT-R certified NISSAN dealer).
NO>>Repair or replace error-detected parts.