CONSULT‐III DATA MONITOR REFERENCE VALUES

Monitor item | Condition | Value/Status
COMP REQ SIG | Engine: Run at idle after warming up | A/C switch: ON (Compressor operation status) | On
A/C switch: OFF | Off
FAN REQ SIG | Engine: Run at idle after warming up | Blower motor: ON | On
Blower motor: OFF | Off
AMB TEMP SEN | Ignition switch ON | — | −22 – 131°F (−30 – 55°C)
IN‐VEH TEMP | Ignition switch ON | — | −22 – 131°F (−30 – 55°C)
INT TEMP SEN | Ignition switch ON | — | −22 – 131°F (−30 – 55°C)
SUNLOAD SEN | Ignition switch ON | — | 0 – 1045 w/m2
AMB SEN CAL | Ignition switch ON | — | −22 – 131°F (−30 – 55°C)
IN‐VEH CAL | Ignition switch ON | — | −22 – 131°F (−30 – 55°C)
INT TEMP CAL | Ignition switch ON | — | −22 – 131°F (−30 – 55°C)
SUNL SEN CAL | Ignition switch ON | — | 0 – 1045 w/m2
FAN DUTY | Engine: Run at idle after warming up | Blower motor: ON | 25 – 81
Blower motor: OFF | 0
XM | Ignition switch ON | — | −100 – 155
ENG COOL TEMP | Ignition switch ON | — | Values according to coolant temperature
VEHICLE SPEED | Driving | — | Equivalent to speedometer reading

TERMINAL LAYOUT
PHYSICAL VALUES

Terminal No. (Wire color) | Description | Condition | Value (Approx.)
+ | − | Signal name | Input/Output
1 (L) | Ground | CAN - H | Input/Output | — | —
2 (P) | Ground | CAN - L | Input/Output | — | —
10 (L) | Ground | A/C LAN signal | Input/Output | Ignition switch ON |
11 (R) | Ground | Each door motor power supply | — | Ignition switch ON | 12 V
15 (O) | Ground | Sunload sensor signal | Input | — | 0 – 4.8 V Output voltage varies with sunload amount
16 (R) | Ground | Intake sensor signal | Input | — | 0 – 4.8 V Output voltage varies with intake temperature
17 (SB) | Ground | ACC power supply | — | Ignition switch ACC | Battery voltage
19 (B) | Ground | Ground | — | Ignition switch ON | 0 V
20 (G) | Ground | Ignition power supply | — | Ignition switch ON | Battery voltage
24 (O) | Ground | ECV signal | Output |

- Ignition switch ON
- HVAC TEST: MODE 5

32 (L) | Ground | Blower motor control signal | Output |

- Ignition switch ON
- Fan speed: 1st speed (manual)

34 (Y) | Ground | A/C auto amp. connecting recognition signal | Output | Ignition switch ON | 5 V
35 (P) | Ground | Ambient sensor signal | Input | — | 0 – 4.8 V Output voltage varies with ambient temperature
36 (LG) | Ground | In-vehicle sensor signal | Input | — | 0 – 4.8 V Output voltage varies with in-vehicle temperature
37 (O) | Ground | Sensor ground | — | Ignition switch ON | 0 V
39 (B) | Ground | Ground | — | Ignition switch ON | 0 V
40 (Y) | Ground | Battery power supply | — | Ignition switch OFF | Battery voltage