1.PRECONDITIONING ■ WARNING ■ When performing the following procedure, always observe the handling of the fuel. Refer to Removal and Installation (GT-R certified NISSAN dealer). TESTING CONDITION: Before starting component function check, preparation of draining fuel and refilling fuel is required.
Do you have CONSULT-III?
YES>>GO TO 2.
NO>>GO TO 3.
2.PERFORM COMPONENT FUNCTION CHECK
With CONSULT-III
NOTE：
Start from step 10, if it is possible to confirm that the fuel cannot be drained by 30 (7-7/8 US gal, 6-5/8 Imp gal) in advance.

1. Prepare a fuel container and a spare hose.
2. Release fuel pressure from fuel line, refer to Inspection (GT-R certified NISSAN dealer).
3. Remove the fuel feed hose on the fuel level sensor unit.
4. Connect a spare fuel hose where the fuel feed hose was removed.
5. Turn ignition switch OFF and wait at least 10 seconds then turn ON.
6. Select “FUEL LEVEL SE” in “DATA MONITOR” mode with CONSULT-III.
7. Check “FUEL LEVEL SE” output voltage and note it.
8. Select “FUEL PUMP RELAY” in “ACTIVE TEST” mode with CONSULT-III.
9. Touch “ON” and drain fuel approximately 30 (7-7/8 US gal, 6-5/8 Imp gal) and stop it.
10. Check “FUEL LEVEL SE” output voltage and note it.
11. Fill fuel into the fuel tank for 30 (7-7/8 US gal, 6-5/8 Imp gal).
12. Check “FUEL LEVEL SE” output voltage and note it.
13. Confirm whether the voltage changes more than 0.03V during step 7 to 10 and 10 to 12.

Is the inspection result normal?
YES>>INSPECTION END
NO>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
3.PERFORM COMPONENT FUNCTION CHECK
Without CONSULT-III
NOTE：
Start from step 8, if it is possible to confirm that the fuel cannot be drained by 30 (7-7/8 US gal, 6-5/8 Imp gal) in advance.

1. Prepare a fuel container and a spare hose.
2. Release fuel pressure from fuel line. Refer to Inspection (GT-R certified NISSAN dealer).
3. Remove the fuel feed hose on the fuel level sensor unit.
4. Connect a spare fuel hose where the fuel feed hose was removed.
5. Turn ignition switch ON.
6. Drain fuel by 30 (7-7/8 US gal, 6-5/8 Imp gal) from the fuel tank using proper equipment.
7. Confirm that the fuel gauge indication varies.
8. Fill fuel into the fuel tank for 30 (7-7/8 US gal, 6-5/8 Imp gal).
9. Confirm that the fuel gauge indication varies.

Is the inspection result normal?
YES>>INSPECTION END
NO>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).