1.CHECK TAIL LAMP OPERATION IPDM E/R AUTO ACTIVE TEST

1. Activate IPDM E/R auto active test. Refer to Diagnosis Description.
2. Check that the tail lamp is turned ON.

CONSULT-III ACTIVE TEST

1. Select "EXTERNAL LAMPS" of IPDM E/R active test item.
2. With operating the test items, check that the tail lamp is turned ON.

   TAIL | : Tail lamp ON
   Off | : Tail lamp OFF

Is the tail lamp turned ON/OFF?
YES>>Tail lamp circuit is normal.
NO>>Refer to Diagnosis Procedure.