1.PERFORM SELF-DIAGNOSIS With CONSULT-III

1. Turn the ignition switch OFF to ON.
2. Perform self-diagnosis of “E-SUS” and check whether DTC “C1D16” is detected.
   ■ CAUTION ■
   Even when a record exists in the diagnosis history, replace E-SUS control unit.

Is DTC “C1D16” detected?
YES>>Replace E-SUS control unit. Refer to Exploded View (GT-R certified NISSAN dealer).
NO>>Check pin terminal and connection of each harness connector for damage or loose connection. Repair or replace error-detected parts.