1.PERFORM WORK SUPPORT Perform “INSIDE ANT DIAGNOSIS” on “Work Support” of “INTELIGENT KEY”. Refer to CONSULT-III Function (BCM - INTELLIGENT KEY). >>GO TO 2. 2.PERFORM SELF DIAGNOSTIC RESULT
Perform Self Diagnostic result of “BCM”.
Is DTC detected?
YES>>Refer to DTC Logic (instrument center), refer to DTC Logic (console), refer to DTC Logic (luggage room).
NO>>GO TO 3.
3.CHECK PUSH-BUTTON IGNITION SWITCH
Check push-button ignition switch.
Refer to Component Function Check.
Is the inspection normal?
YES>>GO TO 4.
NO>>Repair or replace malfunctioning parts.
4.CONFIRM THE OPERATION
Confirm the operation again.
Is the inspection normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.