REMOVAL

1. Remove the door finisher (driver side).Refer to Removal and Installation.
2. Remove the screws (B).
3. Remove power window main switch finisher (driver side) (2) from door finisher (driver side) using flat-bladed screwdriver (A) etc.

   | : Pawl

   ■ CAUTION ■
   Never fold the pawl of door finisher.
4. Remove power window main switch (1) from power window main switch finisher (driver side) using flat-bladed screwdriver (A) etc.

   | : Pawl

   ■ CAUTION ■
   Never fold the pawl of power window main switch finisher.

NOTE：
The same procedure is also performed for power window sub-switch.
INSTALLATION
Install in the reverse order of removal.