REGULATOR ASSEMBLY Removal

1.Remove the door glass. Refer to Removal and Installation (GT-R certified NISSAN dealer).

2.Remove the mounting nuts and bolts, and then remove the door module base (1).

| : Bolt

3.Disconnect the power window motor harness connector (A).

4.Remove the door finisher bracket (1) using a socket wrench (A).

5.Remove the regulator assembly mounting nut using a socket wrench, and then remove the regulator assembly.

| : Nut

Installation
Install in the reverse order of removal.
NOTE：
Always perform the glass position adjustment.
■ CAUTION ■
The regulator assembly mounting nuts (bottom side) can not be reused. Replace them by new nuts.
Inspection After Removal
Check regulator assembly for the following item. Replace if necessary.

- Wire wear
- Deformation of regulator assembly