1.CHECK AUTO/MANUAL RANGE CHANGE SWITCH Check continuity between A/T shift selector harness connector terminals.

TCM vehicle side harness connector | Condition | Continuity
Connector | Terminal
B20 | 16 | 20 | The shift lever is pressed onto the M position side | Not existed
Other than the above | Existed
16 | 24 | The shift lever is pressed onto the M position side | Existed
Other than the above | Not existed

Is the inspection result normal?
YES >>INSPECTION END
NO >>Repair or replace damaged parts.