1.CHECK THE ILLUMINATION OF THE LOW TIRE PRESSURE WARNING LAMP

1. Turn the ignition switch ON.
   ■ CAUTION ■
   Never start engine.
2. Short-circuit the tire pressure warning check switch connector terminal to the ground.
3. Check that the low tire pressure warning lamp blinking.

Is inspection result normal?
YES>>INSPECTION END
NO>>Perform diagnosis. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).