1.CHECK REAR WINDOW DEFOGGER SWITCH FUNCTION

1. Turn ignition switch ON.
2. Connect CONSULT-III and select “DATA MONITOR” mode.
3. Select “LOAD SIGNAL” and check indication under the following conditions.

   Monitor item | Condition | Indication
   LOAD SIGNAL | Rear window defogger switch | ON | ON
   OFF | OFF

Is the inspection result normal?
YES>>GO TO 2.
NO>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
2.CHECK LIGHTING SWITCH FUNCTION
Check “LOAD SIGNAL” indication under the following conditions.

Monitor item | Condition | Indication
LOAD SIGNAL | Lighting switch | ON at 2nd position | ON
OFF | OFF

Is the inspection result normal?
YES>>GO TO 3.
NO>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
3.CHECK HEATER FAN CONTROL SWITCH FUNCTION
Select “HEATER FAN SW” and check indication under the following conditions.

Monitor item | Condition | Indication
HEATER FAN SW | Heater fan control switch | ON | ON
OFF | OFF

Is the inspection result normal?
YES>>INSPECTION END
NO>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).