GENERAL SPECIFICATIONS

Cylinder arrangement | V-6
Displacement　cm3 (cu in) | 3,799 (231.815)
Bore and stroke　mm (in) | 95.5×88.4 (3.760×3.480)
Valve arrangement | DOHC
Firing order | 1-2-3-4-5-6
Number of piston rings | Compression |  | 2
Oil |  | 1
Number of main bearings | 4
Compression ratio | 9.0
Compression pressure kPa (kg/cm2, psi)/200 rpm | Standard |  | 970 (9.89, 141)
Minimum |  | 800 (8.16, 116)
Differential limit between cylinders | 100 (1.02, 14.5)
Cylinder number |
Valve timing : Intake valve : Exhaust valve |
Unit: degree
a | b | c | d | e | f
248 | 238 | 5 ATDC (41 BTCD) | 63 ABDC (17 ABDC) | 9 ATDC | 59 BBDC
( ) : Valve timing control “ON”