1.CHECK “HAZARD ANSWER BACK” SETTING IN “WORK SUPPORT” Check “HAZARD ANSWER BACK” setting in “WORK SUPPORT”. Refer to CONSULT-III Function (BCM - INTELLIGENT KEY). Is the inspection result normal? YES>>GO TO 2.
NO>>Set “HAZARD ANSWER BACK” setting in “WORK SUPPORT”.
2.CHECK “HORN WITH KEYLESS LOCK” SETTING IN “WORK SUPPORT”.
Check “HORN WITH KEYLESS LOCK” setting in “WORK SUPPORT”.
Refer to CONSULT-III Function (BCM - INTELLIGENT KEY).
Is the inspection result normal?
YES>>GO TO 3.
NO>>Set “HORN WITH KEYLESS LOCK” setting in “WORK SUPPORT”.
3.CHECK HAZARD FUNCTION
Check hazard function.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 4.
NO>>Repair or replace the malfunctioning parts.
4.CHECK HORN FUNCTION
Check horn function.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 5.
NO>>Repair or replace the malfunctioning parts.
5.CONFIRM THE OPERATION
Confirm the operation again.
Is the result normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.