For RH side curtain air bag module, crash is judged by main “G” sensor output signal (left side: LH satellite sensor, right side: RH satellite sensor) and safing algorithm (in air bag diagnosis sensor unit). OPERATION In case of side collision whose acceleration exceeds the specified level, the ignition materials are ignited by electric ignition system. The system burns the gas generating materials resulting in a chemical reaction. This generates hot gases that flow into the air bag through a filter and expand the bag.
STRUCTURE
LH side curtain air bag module mainly consists of air bag and inflator that inflates air bag.
INSTALLATION
LH side curtain air bag module is installed on the roof side with fixed bolts.