Measurement Dimensions marked with ″*″ indicate symmetrically identical dimensions on both the right and left hand of the vehicle.

Unit: mm (in) |  |  |  |
| : Vehicle front |  |  |  |
| : Bolt head |  |  |  |

Unit: mm (in) |  |  |  |
| : Vehicle front |  |  |  |

«Front and rear dimension not shown in the figure»

Unit: mm (in)
| Point | Dimension | Memo |  | Point | Dimension | Memo |  | Point | Dimension | Memo |
| G - F | 231.0 (9.094)* |  |  | H - M | 638.5 (25.138)* |  |  |  |  |  |
| H - J | 121.0 (4.764)* |  | H - Q | 1505.0 (59.252)* |  |  |  |  |

«Width dimension not shown in the figure»

Unit: mm (in)
| Point | Dimension | Memo |  | Point | Dimension | Memo |  | Point | Dimension | Memo |
| F - f | 810.0 (31.890) |  |  | M - m | 1372.0 (54.016) |  |  |  |  |  |
| J - j | 1445.2 (56.898) |  | Q - q | 1022.0 (40.236) |  |  |  |  |

«Opposite angle dimension not shown in the figure»

Unit: mm (in)
| Point | Dimension | Memo |  | Point | Dimension | Memo |  | Point | Dimension | Memo |
| G - f | 672.0 (26.457) |  |  | H - j | 1014.8 (39.953)* |  |  | H - q | 1702.5 (67.027)* |  |
| g - F | 748.5 (29.468) |  | H - m | 1162.1 (45.752)* |  |  |  |  |

Measurement Points

| : Vehicle front |  |  |  |

Unit: mm (in)
Point | Remarks | Point | Remarks
A, a, E, e | Front side member location hole center φ16 (0.63) | K, k | Transmission mounting installing bolt head
B, b, D, d | Front suspension member installing bolt head | M, m, O, o, P, p | Rear suspension member installing bolt head
C, c | Front side member measurement hole center φ14 (0.55) | R, r | Rear side member extension location hole center 18×16 (0.71×0.63)
F, f | Front side member extension location hole center φ16 (0.63) | S, s | Rear strut installing hole center φ30 (1.18)
G, g, H, h | Center front floor location hole center φ12 (0.47) | T, t, U, u | Front strut housing upper link installing hole center φ12.5 (0.492)
J, j | Inner sill measurement hole center φ9 (0.35) | V, v | Steering member installing hole center φ13 (0.51)
N, n, Q, q | Rear side member location hole center N, n: φ16 (0.63) Q, q: φ12 (0.47) | W | Tunnel stay mounting hole center φ14 (0.55)