MOUNTING INSPECTION Check the mounting conditions (looseness, backlash) of each component and component conditions (wear, damage) are normal. BALL JOINT AXIAL END PLAY

1.Set front wheels in a straight-ahead position.

2.Place an iron bar or equivalent between transverse link or upper link and steering knuckle.

3.Measure axial end play by playing it up and down.

Axial end play | : Refer to Ball Joint (GT-R certified NISSAN dealer).

■ CAUTION ■

- Never depress brake pedal when measuring.
- Never perform with tires on level ground.
- Be careful not to damage ball joint boot. never damage the installation position by applying excessive force.

SHOCK ABSORBER
Check for oil leakage and damage. Replace it if necessary.