1.CHECK PARKING BRAKE SWITCH

1. Turn the ignition switch OFF.
2. Disconnect the parking brake switch connector.
3. Check for continuity between the parking brake switch connector and the ground.

   Parking brake switch | Measuring condition | Continuity
   (+) | (-)
   1 | Ground | Parking brake applied | Existed
   Parking brake released | Not exist

YES>>INSPECTION END
NO>>Replace the parking brake switch.