DTC DETECTION LOGIC NOTE：

- If DTC B2606 is displayed with DTC U1000, first perform the trouble diagnosis for DTC U1000. Refer to DTC Logic.
- If DTC B2606 is displayed with DTC U1010, first perform the trouble diagnosis for DTC U1010. Refer to DTC Logic.

DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
B2606 | S/L RELAY | BCM detects that there is a mismatch between the following statuses.

- Steering lock unit ON signal transmitted by IPDM E/R
- The steering lock unit status feedback

Steering lock relay (Built into IPDM E/R)

DTC CONFIRMATION PROCEDURE
1.PERFORM DTC CONFIRMATION PROCEDURE

1. Turn ignition switch ON under the following conditions.

- Shift lever is in the P or N position.
- Do not depress brake pedal.

2. Turn ignition switch OFF.
3. Press driver side door switch and wait for at least 1 second.
4. Check “Self diagnostic result” with CONSULT-III.

Is DTC detected?
YES>>Go to Diagnosis Procedure.
NO>>INSPECTION END