1.CHECK BATTERY TERMINALS CONNECTION Check if battery terminals are clean and tight. Is the inspection result normal? YES>>GO TO 2. NO>>Repair battery terminals connection.
2.CHECK FUSE
Check for blown fuse and fusible link.

Unit | Power source (Power supply terminals) | Fuse No.
Alternator | Battery (“S” terminal) | 38
Combination meter | Ignition switch ON (“L” terminal) | 4

Is the inspection result normal?
YES>>GO TO 3.
NO>>Be sure to eliminate the cause of malfunction before installing new fuse.
3.CHECK DRIVE BELT TENSION
Check drive belt tension. Refer to Checking.
Is the inspection result normal?
YES>>INSPECTION END
NO>>Repair as needed.