REMOVAL

1.Remove preset switch. Refer to Exploded View (BASE AUDIO WITH NAVIGATION) or Exploded View (BOSE AUDIO WITH NAVIGATION).

2.Remove set-up switch assembly. Refer to Exploded View.

3.Remove cluster lid C (lower). Refer to Exploded View.

4.Remove mounting screws (A).

5.Disconnect A/C auto amp. harness connector, and then remove A/C auto amp. (1) together with A/C auto amp. bracket.

6.Remove mounting screws (A), and then remove A/C auto amp. bracket from A/C auto amp. (1).

INSTALLATION
Installation is basically the reverse order of removal.