DTC DETECTION LOGIC

DTC | Display item | Malfunction detected condition | Possible cause
C1113 | G-SENSOR | Decel G sensor is malfunctioning. |

- Harness or connector
- ABS actuator and electric unit (control unit)
- Yaw rate/side/decel G sensor

C1145 | YAW RATE SENSOR |

- Yaw rate sensor is malfunctioning.
- Yaw rate/side/decel G sensor power voltage is outside the standard.
- Yaw rate/side/decel G sensor signal line is open or shorted.

C1146 | SIDE G-SEN CIRCUIT | Side G sensor is malfunctioning.

DTC CONFIRMATION PROCEDURE
1.DTC REPRODUCTION PROCEDURE

1. Turn the ignition switch ON.
2. Perform self-diagnosis for “ABS” with CONSULT-III.

Is DTC “C1113”, “C1145” or “C1146” detected?
YES>>Proceed to diagnosis procedure. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END