NOTE：

- The details of time display are as follows.

- CRNT: A malfunction is detected now.
- PAST: A malfunction was detected in the past.

- IGN counter is displayed on FFD (Freeze Frame data).

- The number is 0 when is detected now.
- The number increases like 1 → 2 ··· 38 → 39 after returning to the normal condition whenever IGN OFF → ON.
- The number is fixed to 39 until the self-diagnosis results are erased if it is over 39.

×: Applicable
CONSULT display | Fail-safe | Refer to
No DTC is detected. further testing may be required. | — | —
U1000: CAN COMM CIRCUIT | × | Description
B2098: IGN RELAY ON | × | Description
B2099: IGN RELAY OFF | — | Description
B2108: STRG LCK RELAY ON | — | Description
B2109: STRG LCK RELAY OFF | — | Description
B210A: STRG LCK STATE SW | — | Description
B210B: START CONT RLY ON | — | Description
B210C: START CONT RLY OFF | — | Description
B210D: STARTER RELAY ON | — | Description
B210E: STARTER RELAY OFF | — | Description
B210F: INTRLCK/PNP SW ON | — | Description
B2110: INTRLCK/PNP SW OFF | — | Description