When the control unit is replace, initialization is necessary. If any of the following operations are performed, the initialization is necessary as well as when the control unit is disconnected.

1.Initial connection or reconnection of battery terminal.

2.Removal and installation of power window regulator.

3.Removal and installation of power window motor.

4.When the power supply to power window switches and motor shuts off for any reason while power widow is being operated.

5.Fuse blowout and replacement of fuse for the power window power supply.

6.Removal and installation of door glass or adjustment of door glass.

■ CAUTION ■
The following specified operations are not performed under the non-initialized condition.

- AUTO UP operation
- Anti-pinch function
- Automatic window adjusting function
- Retained power operation