REMOVAL

1.Remove the front wiper arm. Refer to Exploded View.

2.Remove the cowl top cover. Refer to Exploded View.

3.Remove the font wiper drive assembly mounting bolts.

4.Disconnect the front wiper motor connector.

5.Remove the front wiper drive assembly from the vehicle.

INSTALLATION

1.Install the front wiper drive assembly to the vehicle.

2.Connect the front wiper motor connector.

3.Operate the front wiper to move it to the auto stop position.

4.Install the cowl top cover. Refer to Exploded View.

5.Install the front wiper arms. Refer to Exploded View.