1.CHECK PARKING BRAKE WARNING LAMP

1. Start the engine.
2. Check the operation of the brake warning lamp by operating the parking brake.

   When parking brake is applied | : ON
   When parking brake is released | : OFF

Is the inspection result normal?
YES>>Replace the combination meter.
NO>>GO TO 2.
2.CHECK PARKING BRAKE SWITCH SIGNAL CIRCUIT
Perform a check for the parking brake switch signal circuit. Refer to Diagnosis Procedure.
Is the inspection result normal?
YES>>GO TO 3.
NO>>Repair harness or connector.
3.CHECK PARKING BRAKE SWITCH UNIT
Perform a unit check for the parking brake switch. Refer to Component Inspection.
Is the inspection result normal?
YES>>Replace the combination meter.
NO>>Replace the parking brake switch.