DESCRIPTION

- If the ignition switch is turned to the OFF position while the REC switch is set to ON (manual REC), “Perform the memory” or “Do not perform the memory” of REC switch ON (manual REC) condition can be selected.
- If “Perform the memory” was set, the REC switch will be ON (manual REC) when turning the ignition switch to the ON position again.
- If “Do not perform the memory” was set, the air inlets will be controlled automatically when turning the ignition switch to the ON position again.

HOW TO SET
With CONSULT-III
Perform the “REC MEMORY SET” of HVAC work support item.

Work support items | Display | Setting
REC MEMORY SET | WITHOUT (initial status) | Perform the memory of manual REC
WITH | Do not perform the memory of manual REC (auto control)

NOTE：
When the battery cable is disconnected from the negative terminal or when the battery voltage becomes 10 V or less, the setting of the REC switch memory function may be cancelled.