CALIBRATION OF VALVE ■ CAUTION ■

- To calibrate valve, always use CONSULT-III.
  (Calibration cannot be done without CONSULT-III)
- Always perform the valve calibration after finishing the pressure sensor calibration. (If the pressure sensor calibration is not completed, the valve calibration cannot be performed.)
- Perform the valve calibration with the vehicle stopped.
- Never depress the brake pedal during the valve calibration.

1.PERFORM THE PRESSURE SENSOR CALIBRATION
Perform the pressure sensor calibration. Refer to Special Repair Requirement (GT-R certified NISSAN dealer).
>>GO TO 2.
2.PERFORM THE CALIBRATION OF VALVE

1. Select “ABS”, “WORK SUPPORT” and “VALVE CALIBRATION” in order with CONSULT-III.
2. Select “START”.
3. After approximately 40 seconds, select “END”.
4. Turn the ignition switch OFF, then turn it ON again.
   ■ CAUTION ■
   Always perform the above operation.

>> GO TO 3.
3.ERASE THE SELF-DIAGNOSIS MEMORY
Erase self-diagnosis memories for “ABS” with CONSULT-III. Refer to CONSULT-III Function (GT-R certified NISSAN dealer).
Are the memories erased?
YES>>INSPECTION END
NO>>Check the items indicated by the self-diagnosis.