1.CHECK TIRE PRESSURE SIGNAL With CONSULT-III

1. Check and adjust the tire pressure for all wheels. Refer to Tire.
2. Perform transmitter ID registration for all wheels. Refer to Transmitter ID Registration Procedure.
3. Within 15 minutes use the CONSULT-III “DATA MONITOR” to read the tire pressure for all wheels.
4. Check that “DATA MONITOR” displays tire pressure of 438.60 kPa (4.47kg/cm2, 63.60 psi).

Is the inspection result normal?
YES>>Replace the malfunctioning transmitter.
NO>>GO TO 2.
2.CHECK TPMS
Check the transmitters. Refer to Component Inspection (GT-R certified NISSAN dealer).
Is the inspection result normal?
YES>>INSPECTION END
NO>>Perform trouble diagnosis of the low tire pressure warning control unit. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).